(export (version "E")
  (design
    (source "/home/synthesis/Desktop/LABS/Electronics/PCB/Power_Supply_Kicad_like_pro_v1_learning_prj/Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch")
    (date "2026-02-21T06:27:09-0700")
    (tool "Eeschema 9.0.6+b1")
    (textvar (name "Athor") "Sinus")
    (textvar (name "Corp") "SocioCybereeng")
    (textvar (name "URL") "sociocyber.site/pcb/Arduino_modules/PowerSupply_ACDC_DC_1_0_0")
    (textvar (name "Version") "v1")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title "Power_Supply_v1")
        (company)
        (rev "1")
        (date "2026-02-17")
        (source "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch")
        (comment (number "1") (value "Arduino modules"))
        (comment (number "2") (value "Power your shemes with DC 5V"))
        (comment (number "3") (value "ACDC-DC-1.0.0"))
        (comment (number "4") (value "Input voltage: 7V-12V AC/DC power"))
        (comment (number "5") (value "Output voltage: 5V DC currect"))
        (comment (number "6") (value "'SocioCyber'"))
        (comment (number "7") (value "https://sociocyber.site/pcb/Arduino_modules/PowerSupply_ACDC_DC_1_0_0.git"))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "C1")
      (value "470uF")
      (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm")
      (datasheet "~")
      (description "Polarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "Polarized capacitor"))
      (libsource (lib "Device") (part "C_Polarized") (description "Polarized capacitor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "CP_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "63339ccc-c9f0-46ec-af42-67478d761dc3"))
    (comp (ref "C2")
      (value "47uF")
      (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
      (datasheet "~")
      (description "Polarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "Polarized capacitor"))
      (libsource (lib "Device") (part "C_Polarized") (description "Polarized capacitor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "CP_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "0640b486-d51b-48b5-bd11-2440e29413a5"))
    (comp (ref "D1")
      (value "1N4007")
      (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
      (datasheet "http://www.vishay.com/docs/88503/1n4001.pdf")
      (description "1000V 1A General Purpose Rectifier Diode, DO-41")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
        (field (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf")
        (field (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (libsource (lib "Diode") (part "1N4007") (description "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*DO?41*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "82119dce-8560-43e4-8530-c2e54ce440f0"))
    (comp (ref "D2")
      (value "1N4007")
      (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
      (datasheet "http://www.vishay.com/docs/88503/1n4001.pdf")
      (description "1000V 1A General Purpose Rectifier Diode, DO-41")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
        (field (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf")
        (field (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (libsource (lib "Diode") (part "1N4007") (description "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*DO?41*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "18031368-699d-4843-9601-4574ee5aa476"))
    (comp (ref "D3")
      (value "1N4007")
      (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
      (datasheet "http://www.vishay.com/docs/88503/1n4001.pdf")
      (description "1000V 1A General Purpose Rectifier Diode, DO-41")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
        (field (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf")
        (field (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (libsource (lib "Diode") (part "1N4007") (description "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*DO?41*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "7c1710bc-fb8d-43f3-bef9-89f9bcff4a79"))
    (comp (ref "D4")
      (value "1N4007")
      (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
      (datasheet "http://www.vishay.com/docs/88503/1n4001.pdf")
      (description "1000V 1A General Purpose Rectifier Diode, DO-41")
      (fields
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
        (field (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf")
        (field (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (libsource (lib "Diode") (part "1N4007") (description "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "diode"))
      (property (name "ki_fp_filters") (value "D*DO?41*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "da2c8add-24a0-41ea-aa42-107974314537"))
    (comp (ref "D5")
      (value "LED")
      (footprint "LED_THT:LED_D5.0mm")
      (datasheet "~")
      (description "Light emitting diode")
      (fields
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "LED_THT:LED_D5.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode"))
      (libsource (lib "Device") (part "LED") (description "Light emitting diode"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "LED diode"))
      (property (name "ki_fp_filters") (value "LED* LED_SMD:* LED_THT:*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "1f8062e0-ab74-4b22-bee7-55146a76f1f2"))
    (comp (ref "D6")
      (value "LED")
      (footprint "LED_THT:LED_D5.0mm")
      (datasheet "~")
      (description "Light emitting diode")
      (fields
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Footprint") "LED_THT:LED_D5.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode"))
      (libsource (lib "Device") (part "LED") (description "Light emitting diode"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "LED diode"))
      (property (name "ki_fp_filters") (value "LED* LED_SMD:* LED_THT:*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "4fad0547-1479-4833-b686-43e2166b3fab"))
    (comp (ref "J1")
      (value "Barrel_Jack_Switch")
      (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal")
      (datasheet "~")
      (description "DC Barrel Jack with an internal switch")
      (fields
        (field (name "Footprint") "Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal")
        (field (name "Datasheet") "~")
        (field (name "Description") "DC Barrel Jack with an internal switch"))
      (libsource (lib "Connector") (part "Barrel_Jack_Switch") (description "DC Barrel Jack with an internal switch"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "DC power barrel jack connector"))
      (property (name "ki_fp_filters") (value "BarrelJack*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "bafa996f-bab7-4833-b07b-c1446d1951f8"))
    (comp (ref "J2")
      (value "Conn_02x02_Odd_Even")
      (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical")
      (datasheet "~")
      (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_02x02_Odd_Even") (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_2x??_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "6d5c671a-c19f-4178-a337-942c5530993d"))
    (comp (ref "J3")
      (value "Conn_02x02_Odd_Even")
      (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical")
      (datasheet "~")
      (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_02x02_Odd_Even") (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_2x??_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "d59ff6c8-3b4a-468e-8ae5-659c1f46ec28"))
    (comp (ref "R1")
      (value "560R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "56400cf0-7dcf-4f95-9792-3086e0eca5f0"))
    (comp (ref "R2")
      (value "560R")
      (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "abd324b9-6b09-421c-8291-0c173e5e47c6"))
    (comp (ref "SW1")
      (value "SW_DPDT_x2")
      (footprint "digikey-footprints:Switch_Slide_11.6x4mm_EG1218")
      (datasheet "https://ex.com")
      (description "Switch, dual pole double throw, separate symbols")
      (fields
        (field (name "Footprint") "digikey-footprints:Switch_Slide_11.6x4mm_EG1218")
        (field (name "Datasheet") "https://ex.com")
        (field (name "Description") "Switch, dual pole double throw, separate symbols"))
      (libsource (lib "Switch") (part "SW_DPDT_x2") (description "Switch, dual pole double throw, separate symbols"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "switch dual-pole double-throw DPDT spdt ON-ON"))
      (property (name "ki_fp_filters") (value "SW*DPDT*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "92eda9bf-6862-4489-bb65-160f6633e66b"))
    (comp (ref "U1")
      (value "LM7805_TO220")
      (footprint "Package_TO_SOT_THT:TO-220-3_Vertical")
      (datasheet "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF")
      (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (fields
        (field (name "Footprint") "Package_TO_SOT_THT:TO-220-3_Vertical")
        (field (name "Datasheet") "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF")
        (field (name "Description") "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"))
      (libsource (lib "Regulator_Linear") (part "LM7805_TO220") (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "Power_Supply_Kicad_like_pro_v1_learning_prj.kicad_sch"))
      (property (name "ki_keywords") (value "Voltage Regulator 1A Positive"))
      (property (name "ki_fp_filters") (value "TO?220*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "3d3290d1-b5a6-4f70-b7aa-1f3c897b75bf")))
  (libparts
    (libpart (lib "Connector") (part "Barrel_Jack_Switch")
      (description "DC Barrel Jack with an internal switch")
      (docs "~")
      (footprints
        (fp "BarrelJack*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Barrel_Jack_Switch")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "DC Barrel Jack with an internal switch"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))
        (pin (num "3") (name "") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_02x02_Odd_Even")
      (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_2x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_02x02_Odd_Even")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))))
    (libpart (lib "Device") (part "C_Polarized")
      (description "Polarized capacitor")
      (docs "~")
      (footprints
        (fp "CP_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C_Polarized")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Polarized capacitor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "LED")
      (description "Light emitting diode")
      (docs "~")
      (footprints
        (fp "LED*")
        (fp "LED_SMD:*")
        (fp "LED_THT:*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "LED")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode")
        (field (name "Sim.Pins") "1=K 2=A"))
      (pins
        (pin (num "1") (name "K") (type "passive"))
        (pin (num "2") (name "A") (type "passive"))))
    (libpart (lib "Device") (part "R")
      (description "Resistor")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Diode") (part "1N4007")
      (description "1000V 1A General Purpose Rectifier Diode, DO-41")
      (docs "http://www.vishay.com/docs/88503/1n4001.pdf")
      (footprints
        (fp "D*DO?41*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "1N4007")
        (field (name "Footprint") "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
        (field (name "Datasheet") "http://www.vishay.com/docs/88503/1n4001.pdf")
        (field (name "Description") "1000V 1A General Purpose Rectifier Diode, DO-41")
        (field (name "Sim.Device") "D")
        (field (name "Sim.Pins") "1=K 2=A"))
      (pins
        (pin (num "1") (name "K") (type "passive"))
        (pin (num "2") (name "A") (type "passive"))))
    (libpart (lib "Regulator_Linear") (part "LM7805_TO220")
      (description "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
      (docs "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF")
      (footprints
        (fp "TO?220*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "LM7805_TO220")
        (field (name "Footprint") "Package_TO_SOT_THT:TO-220-3_Vertical")
        (field (name "Datasheet") "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF")
        (field (name "Description") "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220"))
      (pins
        (pin (num "1") (name "VI") (type "power_in"))
        (pin (num "2") (name "GND") (type "power_in"))
        (pin (num "3") (name "VO") (type "power_out"))))
    (libpart (lib "Switch") (part "SW_DPDT_x2")
      (description "Switch, dual pole double throw, separate symbols")
      (docs "~")
      (footprints
        (fp "SW*DPDT*"))
      (fields
        (field (name "Reference") "SW")
        (field (name "Value") "SW_DPDT_x2")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Switch, dual pole double throw, separate symbols"))
      (pins
        (pin (num "1") (name "A") (type "passive"))
        (pin (num "2") (name "B") (type "passive"))
        (pin (num "3") (name "C") (type "passive"))
        (pin (num "4") (name "A") (type "passive"))
        (pin (num "5") (name "B") (type "passive"))
        (pin (num "6") (name "C") (type "passive")))))
  (libraries
    (library (logical "Connector")
      (uri "/usr/share/kicad/symbols//Connector.kicad_sym"))
    (library (logical "Connector_Generic")
      (uri "/usr/share/kicad/symbols//Connector_Generic.kicad_sym"))
    (library (logical "Device")
      (uri "/usr/share/kicad/symbols//Device.kicad_sym"))
    (library (logical "Diode")
      (uri "/usr/share/kicad/symbols//Diode.kicad_sym"))
    (library (logical "Regulator_Linear")
      (uri "/usr/share/kicad/symbols//Regulator_Linear.kicad_sym"))
    (library (logical "Switch")
      (uri "/usr/share/kicad/symbols//Switch.kicad_sym")))
  (nets
    (net (code "1") (name "/V-") (class "Power")
      (node (ref "C1") (pin "2") (pintype "passive"))
      (node (ref "C2") (pin "2") (pintype "passive"))
      (node (ref "D3") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "D4") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "D5") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "D6") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "J2") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "J2") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "J3") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "J3") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "2") (pinfunction "GND") (pintype "power_in")))
    (net (code "2") (name "/V1") (class "Power")
      (node (ref "D1") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "D3") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "J1") (pin "1") (pintype "passive")))
    (net (code "3") (name "/V2") (class "Power")
      (node (ref "D2") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "D4") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "J1") (pin "2") (pintype "passive")))
    (net (code "4") (name "/Vin") (class "Power")
      (node (ref "C1") (pin "1") (pintype "passive"))
      (node (ref "D1") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "D2") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "U1") (pin "1") (pinfunction "VI") (pintype "power_in")))
    (net (code "5") (name "/Vout1") (class "Power")
      (node (ref "C2") (pin "1") (pintype "passive"))
      (node (ref "R1") (pin "1") (pintype "passive"))
      (node (ref "SW1") (pin "2") (pinfunction "B") (pintype "passive"))
      (node (ref "U1") (pin "3") (pinfunction "VO") (pintype "power_out")))
    (net (code "6") (name "/Vout1.1") (class "Power")
      (node (ref "J2") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J2") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J3") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J3") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "R2") (pin "2") (pintype "passive"))
      (node (ref "SW1") (pin "1") (pinfunction "A") (pintype "passive")))
    (net (code "7") (name "Net-(D5-A)") (class "Default")
      (node (ref "D5") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "R1") (pin "2") (pintype "passive")))
    (net (code "8") (name "Net-(D6-A)") (class "Default")
      (node (ref "D6") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "R2") (pin "1") (pintype "passive")))
    (net (code "9") (name "unconnected-(J1-Pad3)") (class "Default")
      (node (ref "J1") (pin "3") (pintype "passive+no_connect")))
    (net (code "10") (name "unconnected-(SW1A-C-Pad3)") (class "Default")
      (node (ref "SW1") (pin "3") (pinfunction "C") (pintype "passive+no_connect")))))